

	
	Project: XYZ 
Project No.: ABC 
	
	TEST PIT # 12345 
Location: India 
	Page 1 of 1 

	
	Co-ordinates (m):  1223456E; 234567N Ground Elevation (m): 1092 
	Facility: Test Site	Start Date: 7 Jan 2022 
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)Finish Date: 10 Jan 2023 Excavator: VOLVO EC290B 


	
	Survey Method: Handheld GPS	Operator: Cobalt 
Datum: xyz 
	Final Depth Of Pit (m): 4.5 
Logged by: SB 
Reviewed by: SBJ 
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	G1 
G2 
	
	TOPSOIL 
sandy, brown, moist, organics, roots. 
From 0.2 m to 0.25 m, Ash: fine grained sand, poorly graded, white to grey, moist, no cementation. 
SAND 
fine to medium grained, silty, some fine to coarse gravel, trace clay, trace cobbles, poorly graded, compact to dense, subangular, olive grey to brown, moist, homogeneous, weak 
cementation, trace oxide staining, maximum particle size: 0.25 m diameter. 
[TILL] 
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	CLAY AND SAND 
silty, trace fine gravel, trace cobbles, trace boulders, fines are of low plasticity, stiff to very stiff, olive grey to greenish brown, drier than plastic limit, homogeneous, weak 
cementation, sand is fine to medium grained, slow dilatancy, maximum particle size: 0.35 m diameter. 
[TILL] 
Note: bedrock in north test pit wall at 3.5 m and in the test pit base at 4.0 m. 
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	
	
	
	

	
	
	
	
	
	SCHIST 
fine grained, foliated, weak, dark grey with oxide staining on foliations, can rip into sand to cobble sized fragments with excavator bucket. 
End of test pit at 4.5 m. 
Notes: 
1. Test pit terminated at target depth. 
2. No groundwater seepage encountered. 3. No frozen ground encountered. 
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	Client: ABCDa 
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FARO (TESTPIT)  FARO_SOIL_ROCK.GDL  BGC.GDT 3/10/17
 
)Sample Type 
Sample No. 
Depth (m) 
Symbol 
FARO (TESTPIT)  FARO_SOIL_ROCK.GDL  BGC.GDT 3/10/17 
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